

VLAN Trunks:

This enables devices connected to different switches but in the same VLAN to communicate without going through a router




VLAN keret: (802.1Q)




VLAN létrehozás:




VLAN rendelés porthoz:



VLAN port trunk mode:



Voice VLAN:



DTP – Negotiated Interface Modes

